[Version]
LayoutFile=LAYOUT.INF, layout1.inf, layout2.inf
signature="$CHICAGO$"
Class=MEDIA
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%Philips%
; _OEM_  Enter name of .cat file from WHQL, containing the digital signature.
; _OEM_  The catalog file has to be in the same location as the INF file.
CatalogFile=PhTvTune.cat
DriverVer=10/29/2003, 2.3.1.8

[ControlFlags]
;ExcludeFromSelect=*

[Manufacturer]
%Philips%=Philips

[DestinationDirs]
PhTVTune.CopyDrivers = 10,system32\drivers
;PhTVTune.CopyFindCD=10

[SourceDisksFiles]
PhTVTune.sys=1

[SourceDisksNames]
1=%DiskName%,,


[Philips]
%PhTVTune.DescFM1216ME%=PhTVTune.FM1216ME,STREAM\PhTVFM   		;
%PhTVTune.DescFQ1216ME%=PhTVTune.FQ1216ME,STREAM\PhTVFQ   		;
%PhTVTune.TNF8532BF%=PhTVTune.TNFBF,STREAM\PhTVBF   		;
%PhTVTune.TNF8532DF%=PhTVTune.TNFDF,STREAM\PhTVDF   		;
%PhTVTune.TCL2002MI3%=PhTVTune.TCLMI3,STREAM\PhTMI3   		;
%PhTVTune.TCL2002MB3%=PhTVTune.TCLMB3,STREAM\PhTMB3   		;
%PhTVTune.TCL2002MI1F%=PhTVTune.TCLMI1F,STREAM\PhTMI1F   		;
%PhTVTune.TCL2002N6A%=PhTVTune.TCLN6A,STREAM\PhTN6A   		;
%PhTVTune.TCL2002NJ5%=PhTVTune.TCLNJ5,STREAM\PhTNJ5   		;


[PhTVTune.FM1216ME]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration
AddReg     = PhTVTune.AddReg, FM1216ME.AddReg
CopyFiles  = PhTVTune.CopyDrivers
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.FM1216ME.NT]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration.NT
CopyFiles  = PhTVTune.CopyDrivers
AddReg     = PhTVTune.AddReg, FM1216ME.AddReg
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.FQ1216ME]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration
AddReg     = PhTVTune.AddReg, FQ1216ME.AddReg
CopyFiles  = PhTVTune.CopyDrivers
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.FQ1216ME.NT]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration.NT
CopyFiles  = PhTVTune.CopyDrivers
AddReg     = PhTVTune.AddReg, FQ1216ME.AddReg
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.TNFBF]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration
AddReg     = PhTVTune.AddReg, TNFBF.AddReg
CopyFiles  = PhTVTune.CopyDrivers
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.TNFBF.NT]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration.NT
CopyFiles  = PhTVTune.CopyDrivers
AddReg     = PhTVTune.AddReg, TNFBF.AddReg
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.TNF8532DF]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration
AddReg     = PhTVTune.AddReg, TNFDF.AddReg
CopyFiles  = PhTVTune.CopyDrivers
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.TNFDF.NT]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration.NT
CopyFiles  = PhTVTune.CopyDrivers
AddReg     = PhTVTune.AddReg, TNFDF.AddReg
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.TCLMI3]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration
AddReg     = PhTVTune.AddReg, TCLMI3.AddReg
CopyFiles  = PhTVTune.CopyDrivers
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.TCLMI3.NT]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration.NT
CopyFiles  = PhTVTune.CopyDrivers
AddReg     = PhTVTune.AddReg, TCLMI3.AddReg
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.TCLMB3]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration
AddReg     = PhTVTune.AddReg, TCLMB3.AddReg
CopyFiles  = PhTVTune.CopyDrivers
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.TCLMB3.NT]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration.NT
CopyFiles  = PhTVTune.CopyDrivers
AddReg     = PhTVTune.AddReg, TCLMB3.AddReg
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.TCLMI1F]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration
AddReg     = PhTVTune.AddReg, TCLMI1F.AddReg
CopyFiles  = PhTVTune.CopyDrivers
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.TCLMI1F.NT]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration.NT
CopyFiles  = PhTVTune.CopyDrivers
AddReg     = PhTVTune.AddReg, TCLMI1F.AddReg
KnownFiles = PhTVTune.KnownFiles

;PhTVTune.TCLN6A
[PhTVTune.TCLN6A]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration
AddReg     = PhTVTune.AddReg, TCLN6A.AddReg
CopyFiles  = PhTVTune.CopyDrivers
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.TCLN6A.NT]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration.NT
CopyFiles  = PhTVTune.CopyDrivers
AddReg     = PhTVTune.AddReg, TCLN6A.AddReg
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.TCLNJ5]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration
AddReg     = PhTVTune.AddReg, TCLNJ5.AddReg
CopyFiles  = PhTVTune.CopyDrivers
KnownFiles = PhTVTune.KnownFiles

[PhTVTune.TCLNJ5.NT]
Include    = ks.inf, kscaptur.inf
Needs      = KS.Registration,KSCAPTUR.Registration.NT
CopyFiles  = PhTVTune.CopyDrivers
AddReg     = PhTVTune.AddReg, TCLNJ5.AddReg
KnownFiles = PhTVTune.KnownFiles


;---------------------------------------------------------------
; Registry entries common to all Philips tuner types
;---------------------------------------------------------------

[PhTVTune.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,PhTVTune.sys
HKR,,PageOutWhenUnopened,3,0

; _OEM_  I2C address: "0xc0" : AS (I2C address pin of the tuner to ground), e.g. Proteus board
;                     "0xc2" : AS between 0.2 and 0.3 V  Default value if AS is unconnected
HKR,,Address,,0xc0         ; I2C address

;HKR,,TunerType,,FM1216ME
; _OEM_  For multistandard tuners add the default video standard here (e.g. 0x00000010 for PAL B)
;HKR,,DefaultStandard,, 0x00000001  ; KS_AnalogVideo_NTSC
;HKR,,DefaultStandard,, 0x00000002  ; KS_AnalogVideo_NTSC_MJ
HKR,,DefaultStandard,, 0x00000010  ; KS_AnalogVideo_PAL_B

;HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,FindCD,,"%10%\Welcome.exe"

;For OEM
[FM1216ME.AddReg]
HKR,,TunerType,,FM1216ME

[FQ1216ME.AddReg]
HKR,,TunerType,,FQ1216ME

[TNFBF.AddReg]
HKR,,TunerType,,TNF8532_BF

[TNFDF.AddReg]
HKR,,TunerType,,TNF8532_DF

[TCLMI3.AddReg]
HKR,,TunerType,,TCL2002MI_3

[TCLMB3.AddReg]
HKR,,TunerType,,TCL2002MB_3

[TCLMI1F.AddReg]
HKR,,TunerType,,TCL2002MI_1F

;TCLN6A.AddReg
[TCLN6A.AddReg]
HKR,,TunerType,,TCL2002N_6A

[TCLNJ5.AddReg]
HKR,,TunerType,,TCL2002NJ_5


;---------------------------------------------------------------
; Files to be copied during installation
;---------------------------------------------------------------

[PhTVTune.CopyDrivers]
PhTVTune.sys 


[PhTVTune.KnownFiles]
PhTVTune.sys=safe


;---------------------------------------------------------------
; Interface description
;---------------------------------------------------------------

[PhTVTune.FM1216ME.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.FM1216ME.NT.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.FQ1216ME.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.FQ1216ME.NT.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.TNFBF.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.TNFBF.NT.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.TNFDF.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.TNFDF.NT.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.TCLMI3.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.TCLMI3.NT.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.TCLMB3.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.TCLMB3.NT.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.TCLMI1F.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.TCLMI1F.NT.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

;TCLN6A
[PhTVTune.TCLN6A.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.TCLN6A.NT.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.TCLNJ5.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,

[PhTVTune.TCLNJ5.NT.Interfaces]
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},"GLOBAL",TvTuner,




[TvTuner]
AddReg=TvTuner.AddReg

[TvTuner.AddReg]
HKR,,CLSID,,{266EEE40-6C63-11cf-8A03-00AA006ECB65}
HKR,,FriendlyName,,%DeviceName%


;---------------------------------------------------------------
; Installation details
;---------------------------------------------------------------

[PhTVTune.FM1216ME.NT.Services]
AddService = PhTVTune,0x00000002,PhTVTune.ServiceInstall

[PhTVTune.FQ1216ME.NT.Services]
AddService = PhTVTune,0x00000002,PhTVTune.ServiceInstall

[PhTVTune.TNFBF.NT.Services]
AddService = PhTVTune,0x00000002,PhTVTune.ServiceInstall

[PhTVTune.TNFDF.NT.Services]
AddService = PhTVTune,0x00000002,PhTVTune.ServiceInstall

[PhTVTune.TCLMI3.NT.Services]
AddService = PhTVTune,0x00000002,PhTVTune.ServiceInstall

[PhTVTune.TCLMB3.NT.Services]
AddService = PhTVTune,0x00000002,PhTVTune.ServiceInstall

[PhTVTune.TCLMI1F.NT.Services]
AddService = PhTVTune,0x00000002,PhTVTune.ServiceInstall

;TCLN6A
[PhTVTune.TCLN6A.NT.Services]
AddService = PhTVTune,0x00000002,PhTVTune.ServiceInstall

[PhTVTune.TCLNJ5.NT.Services]
AddService = PhTVTune,0x00000002,PhTVTune.ServiceInstall


[PhTVTune.ServiceInstall]
DisplayName   = %PhTVTune.DescFM1216ME%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %12%\PhTVTune.sys


;---------------------------------------------------------------
; Strings
;---------------------------------------------------------------

[Strings]
SERVICE_KERNEL_DRIVER=1
SERVICE_ERROR_NORMAL=1
SERVICE_AUTO_START=2
SERVICE_DEMAND_START=3


Philips				= "Philips Semiconductors"
captureClassName		= "Sound, video and game controllers"
DiskName			= "TV BABY, WDM TVTuner Install disk"
PhTVTune.DescFM1216ME         	= "TV BABY, WDM TVTuner"
PhTVTune.DescFQ1216ME		= "TV BABY, WDM TVTuner"
PhTVTune.TNF8532BF		= "TV BABY, WDM TVTuner"
PhTVTune.TNF8532DF		= "TV BABY, WDM TVTuner"
PhTVTune.TCL2002MI3		= "TV BABY, WDM TVTuner"
PhTVTune.TCL2002MB3		= "TV BABY, WDM TVTuner"
PhTVTune.TCL2002MI1F		= "TV BABY, WDM TVTuner"
PhTVTune.TCL2002N6A		= "TV BABY, WDM TVTuner"
PhTVTune.TCL2002NJ5		= "TV BABY, WDM TVTuner"
DeviceName                    	= "PhTVTune"


